############################################################

atmega644.name=Sanguino W/ ATmega644P

atmega644.upload.protocol=stk500
atmega644.upload.maximum_size=63488
atmega644.upload.speed=57600

atmega644.bootloader.low_fuses=0xFF
atmega644.bootloader.high_fuses=0x9A
atmega644.bootloader.extended_fuses=0xFF
atmega644.bootloader.path=atmega
atmega644.bootloader.file=ATmegaBOOT_168_atmega644p.hex
#atmega644.bootloader.file=ATmegaBOOT_644P.hex
atmega644.bootloader.unlock_bits=0x3F
atmega644.bootloader.lock_bits=0x0F

atmega644.build.mcu=atmega644p
atmega644.build.f_cpu=16000000L
atmega644.build.core=arduino
atmega644.build.variant=standard
##############################################################

atmega12848m.name=Sanguino W/ ATmega1284p 8mhz

atmega12848m.upload.protocol=stk500
atmega12848m.upload.maximum_size=131072
atmega12848m.upload.speed=19200

atmega1284.bootloader.low_fuses=0xD6
atmega1284.bootloader.high_fuses=0xDA
atmega1284.bootloader.extended_fuses=0xFD
atmega12848m.bootloader.path=atmega
atmega12848m.bootloader.file=ATmegaBOOT_168_atmega1284p_8m.hex
atmega12848m.bootloader.unlock_bits=0x3F
atmega12848m.bootloader.lock_bits=0x0F

atmega12848m.build.mcu=atmega1284p
atmega12848m.build.f_cpu=8000000L
atmega12848m.build.core=arduino
atmega12848m.build.variant=standard

##############################################################

atmega1284.name=Sanguino W/ ATmega1284p 16mhz

atmega1284.upload.protocol=stk500
atmega1284.upload.maximum_size=131072
atmega1284.upload.speed=57600

atmega1284.bootloader.low_fuses=0xD6
atmega1284.bootloader.high_fuses=0xDA
atmega1284.bootloader.extended_fuses=0xFD
atmega1284.bootloader.path=atmega
atmega1284.bootloader.file=ATmegaBOOT_168_atmega1284p.hex
atmega1284.bootloader.unlock_bits=0x3F
atmega1284.bootloader.lock_bits=0x0F

atmega1284.build.mcu=atmega1284p
atmega1284.build.f_cpu=16000000L
atmega1284.build.core=arduino
atmega1284.build.variant=standard
##############################################################

atmega1284m.name=Sanguino W/ ATmega1284p 20mhz

atmega1284m.upload.protocol=stk500
atmega1284m.upload.maximum_size=131072
atmega1284m.upload.speed=57600

atmega1284m.bootloader.low_fuses=0xD6
atmega1284m.bootloader.high_fuses=0xDA
atmega1284m.bootloader.extended_fuses=0xFD
atmega1284m.bootloader.path=atmega
atmega1284m.bootloader.file=ATmegaBOOT_168_atmega1284p.hex
atmega1284m.bootloader.unlock_bits=0x3F
atmega1284m.bootloader.lock_bits=0x0F

atmega1284m.build.mcu=atmega1284p
atmega1284m.build.f_cpu=20000000L
atmega1284m.build.core=arduino
atmega1284m.build.variant=standard
#
