### Version 4.2.82
* Add DONDOLO_DUAL_MOTOR for DONDOLO bowden and dual extruder

### Version 4.2.81
* Fix serial protocol for Repetier Host
* Bug fix

### Version 4.2.8
* Add board folder with files of various board containing the pins
* Add End time on Graphics display when SD print
* Add M35 for upload firmware to Nextion from SD
* Rewrite macros
* Fix M109 so it won't wait for cooling
* Clear code
* Bug fix

### Version 4.2.7
* Add M906 Set motor Currents for ALLIGATOR board
* Add M408 JSON OUTPUT
* Add Cartesian Correction Hysteresis and Zwooble
* Bug fix

### Version 4.2.6
* Bug Fix

### Version 4.2.5
* Big Update
* Add HAL for 8 bit version
* Rewrite Communication
* Rewrite Servo
* Add Color Mixing Extruder

### Version 4.2.4
* Added Abort on endstop hit feature
* Added Purge command G1 P<valor>
* Added M222 T<extruder> S<factor in percent> set density extrude factor percentage for purge

### Version 4.2.3
* Added Filament tot printed in stats
* Overall rewrite

### Version 4.2.2
* Added the possibility to invert the logic for lcd buttons.
* Language files bugfix.
* Fixed a freeze problem during write operations to the SD.
* Re-enabled by default SDSUPPORT for DISCOUNT displays.

### Version 4.2.1
* SDSUPPORT disabled by default.
* General BugFix.

### Version 4.2.0
* Add Dual Extruder DONDOLO.
* Add PID Extrusion Rate Kc in percent.
* New configuration systems (Now you can create a separate file with all configuration and use it in you FW update).
* New namings for file.
* Added more documentation inside configuration file.
* More checks for feature incompatibility during compilation.
* Codeclean.
* General bugfix.
* Removed legacy support for old configuration (Do not use your old configuration files, namings and position for configuration has changed).

### Version 4.1.5
* Added dot for SD write operation.
* Added statistics menu.
* Added an overall configuration file.
* Added M70 gcode for calibrate AC721 current sensor.
* Added documentation for calibrate AC721 current sensor.
* Critical stepper motor frequency bugfix.
* Introduced more intuitive menu tree.
* Added a menu option to fix loose steps from LCD.
* Improved italian translation.
* G28 gcode now support the "B" flag that enable you to come back to the last position of the axis before the homing command. (Used for fix loose steps)
* Implemented FAST_PWM_FAN and FAN_SOFT_PWM also for other fan that can be added in configuration_adv file.
* Added the ability to set a min speed to the fan that can be added in configuration_adv file.
* General bugfix.

### Version 4.1.4
* Add support for Piggy Alligator board
* Add Debug_info. Repetier button info for enabled or disabled, or M111 S2 for enabled and M111 S0 for disabled.
* Improved Topography Auto Bed Level.
* Add Dryrun ABL and verbose width command G29 D or G29 V(0-4).
* Improve Autoconfiguration for Delta printer.
* Add support (test only) for NEXTION HMI LCD.
* Improved firmare test dialog.
* Bugfix for SDCONFIG routine. Now the configuration file will be readed and created only on the root of the SD.
* Improved "Thermal Runaway Protection" now the system will be halted also if the thermistor is missing before the temperature is reached as suggested in Issue #35.
* Improved "Extruder Idle Oozing Prevention" by adding a more efficient way to detect planned movements. Now this feature seems stable and can be used by anyone.
* Bugfix for sdinit.
* Removed tab character from the code.
* Removed some unuseful spacing from the code.

### Version 4.1.3
* Improved support for Delta, SCARA, COREXY & COREXZ kinematics.
* Improved stepper timer for high velocity driver and not.
* Add calibrate surface width DELTA.
* Improved serial comunication width most popular Host.
* Add Acceleration retraction for extruder.
* Add EJerk for extruder.
* Remove limit for virtual extruder to 4. Now width MKR4 or NPr2 is possible have infinite extruder...
* Add M92 T* E (Set step per unit for any extruder).
* Add M203 T* E (Set max feedrate for any extruder).
* Add M204 T* R (Set acc retraction for any extruder).
* Add M205 T* E (Set E Jerk for any extruder).
* Add Slot for G60 & G61.
* G60 Save current position coordinates (all axes, for active extruder).	S<SLOT> - specifies memory slot # (0-based) to save into (default 0).
* G61 Apply/restore saved coordinates to the active extruder. X Y Z E - Value to add at stored coordinates. F<speed> - Set Feedrate. S<SLOT> - specifies memory slot # (0-based) to save into (default 0).

### Version 4.1.2
* Serial message function standardized for a better code style.
* Auto-Create configuration file if not exist.
* FIX for sdcard crash problem during configuration file reading.
* FIX for some undefined SCARA defines.

### Version 4.1.1
* Added Power (Watt) Sensor.
* Added Anti OOZING.
* Add Power Consumation and Power On Time.
* Configurations stored in the SD are updated in real-time (every SD_CFG_SECONDS seconds) also if you remove-insert the sd or you start your printer without the SD card.
* Reduced code size, maybe a lot depending on your configuration.
* Improved support for Delta, SCARA, and COREXY kinematics.
* Move parts of Configuration files to `Conditionals.h` and `SanityCheck.h`.
* Clean up of temperature code.
* Enhanced `G29` with improved grid bed leveling based on Roxy code. See documentation.
* EEPROM layout updated to `V21`.
* Added `M204` travel acceleration options.
* `M204` "`P`" parameter replaces "`S`." "`S`" retained for backward compatibility.
* `M404` "`N`" parameter replaced with "`W`." ("`N`" is for line numbers only).
* Much cleanup of the code.
* Improved support for Cyrillic and accented languages.
* LCD controller knob acceleration.
* Improved compatibility with various sensors, MAX6675 thermocouple.
* Filament runout sensor support.
* Filament width measurement support.
* Support for TMC and L6470 stepper drivers.
* Better support of G-Code `;` comments, `\`, `N` line numbers, and `*` checksums.
* Moved GCode handling code into individual functions per-code.

### Version 4.1.0
* Initial release.
