# OssoPI
====

OssoPI RaspberrPI model 1B+ and 2 I/O expansion board support files

OssoPI RaspberrPI model 1B+ and 2 expansion cape with 8 digital (opto-isolated or non-opto-isolated) inputs
and 8 relays 275VAC@10A.

Osso is shipped with the ability to switch opto-isolated inputs or non-opto-isolated inputs, to better fit user needs.
Docs about how to change input types are on the [project wiki](https://git.nexlab.net/nexlab/OssoPI/wikis/home)

The expansion board has to be powered by a 12VDC connector (9 to 24VDC supported), and it
will power the RaspberryPI from expansion pins ( no needs to give external power
to the RaspberryPI! )

The size of the expansion board is a standard format for 9 units DIN rail mount boxes.

The test files are supposed to run on any linux based os with Rpi.GPIO python library installed,
tested on Raspbian.

For more infos: 
http://www.nexlab.net/

![Osso board](OssoPI1.jpg)
![Osso board](OssoPI2.jpg)

Do you like our cape? donations in Bitcoins are accepted to 1FfyqV2SnrhM5sTwL9jUCt2qPDgCPnwggi

Pin diagram (green dot pins are optional, other required):

![Osso Pin Diagram](OssoPI-PinDiagram.jpg)
