Par Statistics
Total Non-vccgnd Signals=152
Total Non-vccgnd Design Pins=555
Total Non-vccgnd Conns=555
Total Non-vccgnd Timing Constrained Conns=412
Phase 1 CPU=5.4 sec
Phase 2 CPU=6.1 sec
Phase 3 CPU=7.0 sec
Phase 4 CPU=8.8 sec
Phase 5 CPU=9.0 sec
Phase 6 CPU=9.0 sec
Phase 7 CPU=9.0 sec
Phase 8 CPU=9.0 sec
Phase 9 CPU=9.0 sec
Phase 10 CPU=9.0 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=9.0
AvgWirelenPerPin Fanout 3=3.7
AvgWirelenPerPin Fanout 4=1.0
AvgWirelenPerPin Fanout 10=3.2
AvgWirelenPerPin Fanout 50=3.9
AvgWirelenPerPin Fanout 100=0.0
AvgWirelenPerPin Fanout 500=0.0
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.0147