Par Statistics
Total Non-vccgnd Signals=32
Total Non-vccgnd Design Pins=141
Total Non-vccgnd Conns=141
Total Non-vccgnd Timing Constrained Conns=128
Phase 1 CPU=5.1 sec
Phase 2 CPU=5.6 sec
Phase 3 CPU=5.8 sec
Phase 4 CPU=7.4 sec
Phase 5 CPU=7.5 sec
Phase 6 CPU=7.5 sec
Phase 7 CPU=7.5 sec
Phase 8 CPU=7.5 sec
Phase 9 CPU=7.5 sec
Phase 10 CPU=7.5 sec
AvgWirelenPerPin Fanout 1=18.0
AvgWirelenPerPin Fanout 2=11.0
AvgWirelenPerPin Fanout 3=0.0
AvgWirelenPerPin Fanout 4=3.3
AvgWirelenPerPin Fanout 10=14.0
AvgWirelenPerPin Fanout 50=2.0
AvgWirelenPerPin Fanout 100=0.0
AvgWirelenPerPin Fanout 500=0.0
AvgWirelenPerPin Fanout 5000=0.0
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
AvgWirelenPerPin Fanout 100000=0.0
IRR Gamma=1.0025