#
# Configuration generated by Microchip Harmony Configurator (MHC) v1.0.9.2
#     Project name:    http_server
#     Configuration:   pic32mx_eth_sk2_encx24j600
#     Device:          PIC32MX795F512L
#     Harmony version: 1.09
#
#
# from /home/alex/go/src/cesanta.com/mongoose/examples/PIC32/http_server/firmware/http_server.hconfig
#
CONFIG_APP_INSTANCES=1
#
# from $HARMONY_VERSION_PATH/utilities/mhc/config/app_name_idx_gencode.ftl
#
CONFIG_APP_MENU_IDX0=y
CONFIG_APP_NAME_0="app"
CONFIG_APP_AUTO_GENERATE_CODE0=n
#
# from /home/alex/go/src/cesanta.com/mongoose/examples/PIC32/http_server/firmware/http_server.hconfig
#
CONFIG_USE_EXCEPTION_HANDLER=y
CONFIG_EXCEPTION_USE_SYS_DEBUG=y
CONFIG_EXCEPTION_BREAKPOINT=y
#
# from $HARMONY_VERSION_PATH/framework/bluetooth/config/bluetooth.hconfig
#
CONFIG_USE_BLUETOOTH_LIBRARIES=n
#
# from $HARMONY_VERSION_PATH/framework/bootloader/config/bootloader.hconfig
#
CONFIG_USE_BOOTLOADER=n
#
# from $HARMONY_VERSION_PATH/framework/classb/config/classb.hconfig
#
CONFIG_USE_CLASSB=n
#
# from $HARMONY_VERSION_PATH/framework/crypto/config/crypto.hconfig
#
CONFIG_USE_CRYPTO_LIBRARY=n
CONFIG_USE_CRYPTO_LIB=n
#
# from $HARMONY_VERSION_PATH/framework/decoder/config/decoder.hconfig
#
CONFIG_USE_IMAGE_DECODER=n
CONFIG_USE_DECODER=n
#
# from $HARMONY_VERSION_PATH/framework/driver/adc/config/drv_adc.hconfig
#
CONFIG_USE_DRV_ADC=n
#
# from $HARMONY_VERSION_PATH/framework/driver/camera/config/drv_camera.hconfig
#
CONFIG_USE_DRV_CAMERA=n
#
# from $HARMONY_VERSION_PATH/framework/driver/can/config/drv_can.hconfig
#
CONFIG_USE_DRV_CAN=n
#
# from $HARMONY_VERSION_PATH/framework/driver/cmp/config/drv_cmp.hconfig
#
CONFIG_DRV_CVREF_ENABLE=n
CONFIG_USE_DRV_CMP=n
#
# from $HARMONY_VERSION_PATH/framework/driver/encx24j600/config/drv_encx24j600.hconfig
#
CONFIG_DRV_ENCX24J600_USE_DRIVER=y
CONFIG_DRV_ENCX24J600_INSTANCES_NUMBER=1
CONFIG_DRV_ENCX24J600_CLIENT_INSTANCES=1
#
# from $HARMONY_VERSION_PATH/framework/driver/encx24j600/config/drv_encx24j600_idx.ftl
#
CONFIG_DRV_ENCX24J600_IDX0=y
CONFIG_DRV_ENCX24J600_MAC_TX_DESCRIPTORS_IDX0=3
CONFIG_DRV_ENCX24J600_MAC_RX_DESCRIPTORS_IDX0=3
CONFIG_DRV_ENCX24J600_MAX_RX_BUFFER_IDX0=1536
CONFIG_DRV_ENCX24J600_SPI_DRV_INDEX_IDX0=0
CONFIG_DRV_ENCX24J600_SPI_BPS_IDX0=14000000
CONFIG_DRV_ENCX24J600_SPI_SS_PORT_MODULE_IDX0="PORTS_ID_0"
CONFIG_DRV_ENCX24J600_SPI_SS_PORT_CHANNEL_IDX0="PORT_CHANNEL_D"
CONFIG_DRV_ENCX24J600_SPI_SS_PORT_PIN_IDX0="PORTS_BIT_POS_14"
CONFIG_DRV_ENCX24J600_RX_BUFFER_SIZE_IDX0=16384
CONFIG_DRV_ENCX24J600_MAX_FRAME_SIZE_IDX0=1536
CONFIG_DRV_ENCX24J600_MAX_USE_AUTOMATIC_FLOW_CONTROL_IDX0=y
#
# from $HARMONY_VERSION_PATH/framework/driver/enc28j60/config/drv_enc28j60.hconfig
#
CONFIG_DRV_ENC28J60_USE_DRIVER=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tcpip_mac.hconfig
#
CONFIG_TCPIP_USE_ETH_MAC=y
CONFIG_TCPIP_EMAC_TX_DESCRIPTORS=8
CONFIG_TCPIP_EMAC_RX_DESCRIPTORS=6
CONFIG_TCPIP_EMAC_RX_DEDICATED_BUFFERS=4
CONFIG_TCPIP_EMAC_RX_INIT_BUFFERS=0
CONFIG_TCPIP_EMAC_RX_LOW_THRESHOLD=1
CONFIG_TCPIP_EMAC_RX_LOW_FILL=2
CONFIG_TCPIP_EMAC_RX_BUFF_SIZE=1536
CONFIG_TCPIP_EMAC_RX_MAX_FRAME=1536
CONFIG_TCPIP_EMAC_RX_FRAGMENTS=1
CONFIG_TCPIP_EMAC_ETH_FILTER_BCAST_ACCEPT=y
CONFIG_TCPIP_EMAC_ETH_FILTER_MCAST_ACCEPT=y
CONFIG_TCPIP_EMAC_ETH_FILTER_UCAST_ACCEPT=y
CONFIG_TCPIP_EMAC_ETH_FILTER_UCAST_OTHER_ACCEPT=n
CONFIG_TCPIP_EMAC_ETH_FILTER_RUNT_REJECT=y
CONFIG_TCPIP_EMAC_ETH_FILTER_RUNT_ACCEPT=n
CONFIG_TCPIP_EMAC_ETH_FILTER_CRC_ERROR_REJECT=y
CONFIG_TCPIP_EMAC_ETH_FILTER_CRC_ERROR_ACCEPT=n
CONFIG_TCPIP_EMAC_ETH_OF_AUTO_NEGOTIATION=y
CONFIG_TCPIP_EMAC_ETH_OF_FULL_DUPLEX=y
CONFIG_TCPIP_EMAC_ETH_OF_HALF_DUPLEX=y
CONFIG_TCPIP_EMAC_ETH_OF_100=y
CONFIG_TCPIP_EMAC_ETH_OF_10=y
CONFIG_TCPIP_EMAC_ETH_OF_HUGE_PKTS=n
CONFIG_TCPIP_EMAC_ETH_OF_MAC_LOOPBACK=n
CONFIG_TCPIP_EMAC_ETH_OF_PHY_LOOPBACK=n
CONFIG_TCPIP_EMAC_ETH_OF_MDIX_AUTO=y
CONFIG_TCPIP_EMAC_ETH_OF_RMII=n
CONFIG_TCPIP_EMAC_PHY_CONFIG_RMII=n
CONFIG_TCPIP_EMAC_PHY_CONFIG_ALTERNATE=n
CONFIG_TCPIP_EMAC_PHY_CONFIG_AUTO=y
CONFIG_TCPIP_EMAC_PHY_LINK_INIT_DELAY=500
CONFIG_TCPIP_EMAC_PHY_ADDRESS=0
CONFIG_TCPIP_EMAC_MODULE_ID="ETH_ID_0"
CONFIG_TCPIP_EMAC_INTERRUPT_PRIORITY="INT_PRIORITY_LEVEL5"
CONFIG_TCPIP_EMAC_INTERRUPT_SUB_PRIORITY="INT_SUBPRIORITY_LEVEL3"
CONFIG_TCPIP_EMAC_PHY_TYPE="SMSC_LAN8740"
CONFIG_DRV_ETHPHY_INSTANCES_NUMBER=1
CONFIG_DRV_ETHPHY_CLIENTS_NUMBER=1
CONFIG_DRV_ETHPHY_INDEX=1
CONFIG_DRV_ETHPHY_PERIPHERAL_ID=1
CONFIG_DRV_ETHPHY_NEG_INIT_TMO=1
CONFIG_DRV_ETHPHY_NEG_DONE_TMO=2000
CONFIG_DRV_ETHPHY_RESET_CLR_TMO=500
CONFIG_DRV_ETHMAC_INSTANCES_NUMBER=1
CONFIG_DRV_ETHMAC_CLIENTS_NUMBER=1
CONFIG_DRV_ETHMAC_INDEX=1
CONFIG_DRV_ETHMAC_PERIPHERAL_ID=1
CONFIG_DRV_ETHMAC_INTERRUPT_MODE=y
CONFIG_DRV_ETHMAC_POWER_STATE="SYS_MODULE_POWER_RUN_FULL"
#
# from $HARMONY_VERSION_PATH/framework/driver/flash/config/drv_flash.hconfig
#
CONFIG_USE_DRV_FLASH=n
#
# from $HARMONY_VERSION_PATH/framework/driver/gfx/controller/glcd/config/drv_gfx_glcd.hconfig
#
CONFIG_USE_DRV_GFX_GLCD=n
#
# from $HARMONY_VERSION_PATH/framework/driver/gfx/controller/lcc/config/drv_gfx_lcc.hconfig
#
CONFIG_USE_DRV_GFX_LCC=n
#
# from $HARMONY_VERSION_PATH/framework/driver/gfx/controller/otm2201a/config/drv_gfx_otm2201a.hconfig
#
CONFIG_USE_DRV_GFX_OTM2201A=n
#
# from $HARMONY_VERSION_PATH/framework/driver/gfx/controller/ssd1926/config/drv_gfx_ssd1926.hconfig
#
CONFIG_USE_DRV_GFX_SSD1926=n
#
# from $HARMONY_VERSION_PATH/framework/driver/gfx/controller/ssd1289/config/drv_gfx_ssd1289.hconfig
#
CONFIG_USE_DRV_GFX_SSD1289=n
#
# from $HARMONY_VERSION_PATH/framework/driver/gfx/controller/s1d13517/config/drv_gfx_s1d13517.hconfig
#
CONFIG_USE_DRV_GFX_S1D13517=n
#
# from $HARMONY_VERSION_PATH/framework/driver/gfx/display/config/drv_gfx_display.hconfig
#
CONFIG_USE_DRV_GFX_DISPLAY=n
#
# from $HARMONY_VERSION_PATH/framework/driver/i2c/config/drv_i2c.hconfig
#
CONFIG_USE_DRV_I2C=n
#
# from $HARMONY_VERSION_PATH/framework/driver/ic/config/drv_ic.hconfig
#
CONFIG_USE_DRV_IC=n
#
# from $HARMONY_VERSION_PATH/framework/driver/nvm/config/drv_nvm.hconfig
#
CONFIG_USE_DRV_NVM=n
#
# from $HARMONY_VERSION_PATH/framework/driver/oc/config/drv_oc.hconfig
#
CONFIG_USE_DRV_OC=n
#
# from $HARMONY_VERSION_PATH/framework/driver/pmp/config/drv_pmp.hconfig
#
CONFIG_USE_DRV_PMP=n
#
# from $HARMONY_VERSION_PATH/framework/driver/rtcc/config/drv_rtcc.hconfig
#
CONFIG_USE_DRV_RTCC=n
#
# from $HARMONY_VERSION_PATH/framework/driver/sample/config/drv_sample.hconfig
#
CONFIG_USE_DRV_SAMPLE=n
#
# from $HARMONY_VERSION_PATH/framework/driver/sdcard/config/drv_sdcard.hconfig
#
CONFIG_USE_DRV_SDCARD=n
#
# from $HARMONY_VERSION_PATH/framework/driver/spi/config/drv_spi.hconfig
#
CONFIG_DRV_SPI_USE_DRIVER=y
CONFIG_DRV_SPI_DRIVER_MODE="DYNAMIC"
CONFIG_DRV_SPI_USE_ISR_MODE=y
CONFIG_DRV_SPI_USE_POLLED_MODE=n
CONFIG_DRV_SPI_USE_MASTER_MODE=y
CONFIG_DRV_SPI_USE_SLAVE_MODE=n
CONFIG_DRV_SPI_USE_STANDARD_BUFFER_MODE=n
CONFIG_DRV_SPI_USE_ENHANCED_BUFFER_MODE=y
CONFIG_DRV_SPI_USE_8BIT_MODE=y
CONFIG_DRV_SPI_USE_16BIT_MODE=n
CONFIG_DRV_SPI_USE_32BIT_MODE=n
CONFIG_DRV_SPI_USE_DMA=n
CONFIG_DRV_SPI_INSTANCES_NUMBER=1
CONFIG_DRV_SPI_CLIENT_NUMBER=1
CONFIG_DRV_SPI_NUM_ELEMENTS_PER_INSTANCE=10
#
# from $HARMONY_VERSION_PATH/framework/driver/spi/config/drv_spi_idx.ftl
#
CONFIG_DRV_SPI_IDX0=y
CONFIG_DRV_SPI_SPI_ID_IDX0="SPI_ID_1"
CONFIG_DRV_SPI_TASK_MODE_ISR_IDX0=y
CONFIG_DRV_SPI_INT_PRIORITY_IDX0="INT_PRIORITY_LEVEL1"
CONFIG_DRV_SPI_INT_SUB_PRIORITY_IDX0="INT_SUBPRIORITY_LEVEL0"
CONFIG_DRV_SPI_SPI_MODE_MASTER_IDX0=y
CONFIG_DRV_SPI_COMM_WIDTH_8_BIT_IDX0=y
CONFIG_DRV_SPI_BUFFER_ENHANCED_IDX0=y
CONFIG_DRV_SPI_ALLOW_IDLE_RUN_IDX0=n
CONFIG_DRV_SPI_SPI_PROTOCOL_TYPE_IDX0="DRV_SPI_PROTOCOL_TYPE_STANDARD"
CONFIG_DRV_SPI_SPI_CLOCK_IDX0="CLK_BUS_PERIPHERAL_2"
CONFIG_DRV_SPI_BAUD_RATE_IDX0=13333333
CONFIG_DRV_SPI_CLOCK_MODE_IDX0="DRV_SPI_CLOCK_MODE_IDLE_LOW_EDGE_FALL"
CONFIG_DRV_SPI_INPUT_PHASE_IDX0="SPI_INPUT_SAMPLING_PHASE_AT_END"
CONFIG_DRV_SPI_QUEUE_SIZE_IDX0=10
CONFIG_DRV_SPI_RESERVED_JOB_IDX0=1
CONFIG_DRV_SPI_SPI_ID_STATIC_IDX0="SPI_ID_1"
CONFIG_DRV_SPI_SPI_MODE_STATIC_IDX0="DRV_SPI_MODE_MASTER"
CONFIG_DRV_SPI_COMM_WIDTH_STATIC_IDX0="SPI_COMMUNICATION_WIDTH_8BITS"
CONFIG_DRV_SPI_BUFFER_STATIC_IDX0="DRV_SPI_BUFFER_TYPE_ENHANCED"
CONFIG_DRV_SPI_ALLOW_IDLE_RUN_STATIC_IDX0=n
CONFIG_DRV_SPI_SPI_PROTOCOL_TYPE_STATIC_IDX0="DRV_SPI_PROTOCOL_TYPE_STANDARD"
CONFIG_DRV_SPI_FRAME_SYNC_PULSE_STATIC_IDX0="SPI_FRAME_SYNC_PULSE_ON_EVERY_DATA_CHARACTER"
CONFIG_DRV_SPI_FRAME_PULSE_POLARITY_STATIC_IDX0="SPI_FRAME_PULSE_POLARITY_ACTIVE_LOW"
CONFIG_DRV_SPI_FRAME_PULSE_DIRECTION_STATIC_IDX0="SPI_FRAME_PULSE_DIRECTION_OUTPUT"
CONFIG_DRV_SPI_FRAME_PULSE_EDGE_STATIC_IDX0="SPI_FRAME_PULSE_EDGE_PRECEDES_FIRST_BIT_CLOCK"
CONFIG_DRV_SPI_FRAME_PULSE_WIDTH_STATIC_IDX0="SPI_FRAME_PULSE_WIDTH_ONE_CLOCK_WIDE"
CONFIG_DRV_SPI_AUDIO_TRANSMIT_MODE_STATIC_IDX0="SPI_AUDIO_TRANSMIT_STEREO"
CONFIG_DRV_SPI_AUDIO_PROTOCOL_MODE_STATIC_IDX0="SPI_AUDIO_PROTOCOL_I2S"
CONFIG_DRV_SPI_SPI_CLOCK_STATIC_IDX0="CLK_BUS_PERIPHERAL_2"
CONFIG_DRV_SPI_BAUD_RATE_STATIC_IDX0=1000000
CONFIG_DRV_SPI_CLOCK_MODE_STATIC_IDX0="DRV_SPI_CLOCK_MODE_IDLE_LOW_EDGE_RISE"
CONFIG_DRV_SPI_INPUT_PHASE_STATIC_IDX0="SPI_INPUT_SAMPLING_PHASE_IN_MIDDLE"
#
# from $HARMONY_VERSION_PATH/framework/driver/spi/config/drv_spi.hconfig
#
CONFIG_DRV_SPI_STATIC_INSTANCES_NUMBER=0
#
# from $HARMONY_VERSION_PATH/framework/driver/spi_flash/sst25/config/drv_sst25.hconfig
#
CONFIG_USE_DRV_SST25=n
#
# from $HARMONY_VERSION_PATH/framework/driver/spi_flash/sst25vf016b/config/drv_sst25vf016b.hconfig
#
CONFIG_USE_DRV_SST25VF016B=n
#
# from $HARMONY_VERSION_PATH/framework/driver/spi_flash/sst25vf020b/config/drv_sst25vf020b.hconfig
#
CONFIG_USE_DRV_SST25VF020B=n
#
# from $HARMONY_VERSION_PATH/framework/driver/spi_flash/sst25vf064c/config/drv_sst25vf064c.hconfig
#
CONFIG_USE_DRV_SST25VF064C=n
#
# from $HARMONY_VERSION_PATH/framework/driver/sram/config/drv_sram.hconfig
#
CONFIG_USE_DRV_SRAM=n
#
# from $HARMONY_VERSION_PATH/framework/driver/tmr/config/drv_tmr.hconfig
#
CONFIG_USE_DRV_TMR=y
CONFIG_DRV_TMR_DRIVER_MODE="DYNAMIC"
CONFIG_DRV_TMR_CLIENTS_NUMBER=1
CONFIG_DRV_TMR_INTERRUPT_MODE=y
CONFIG_DRV_TMR_INSTANCES_NUMBER=1
#
# from $HARMONY_VERSION_PATH/framework/driver/tmr/config/drv_tmr_idx.ftl
#
CONFIG_DRV_TMR_INST_0=y
CONFIG_DRV_TMR_PERIPHERAL_ID_IDX0="TMR_ID_1"
CONFIG_DRV_TMR_INTERRUPT_PRIORITY_IDX0="INT_PRIORITY_LEVEL1"
CONFIG_DRV_TMR_INTERRUPT_SUB_PRIORITY_IDX0="INT_SUBPRIORITY_LEVEL0"
CONFIG_DRV_TMR_CLOCK_SOURCE_2_IDX0="DRV_TMR_CLKSOURCE_INTERNAL"
CONFIG_DRV_TMR_PRESCALE_IDX0="TMR_PRESCALE_VALUE_256"
CONFIG_DRV_TMR_ASYNC_WRITE_ENABLE_IDX0=n
CONFIG_DRV_TMR_POWER_STATE_IDX0="SYS_MODULE_POWER_RUN_FULL"
#
# from $HARMONY_VERSION_PATH/framework/driver/touch/adc10bit/config/drv_adc10bit.hconfig
#
CONFIG_USE_DRV_TOUCH_ADC10BIT=n
#
# from $HARMONY_VERSION_PATH/framework/driver/touch/ar1021/config/drv_ar1021.hconfig
#
CONFIG_USE_DRV_TOUCH_AR1021=n
#
# from $HARMONY_VERSION_PATH/framework/driver/touch/mtch6301/config/drv_mtch6301.hconfig
#
CONFIG_USE_DRV_TOUCH_MTCH6301=n
#
# from $HARMONY_VERSION_PATH/framework/driver/touch/mtch6303/config/drv_mtch6303.hconfig
#
CONFIG_USE_DRV_TOUCH_MTCH6303=n
#
# from $HARMONY_VERSION_PATH/framework/driver/usart/config/drv_usart.hconfig
#
CONFIG_USE_DRV_USART=y
CONFIG_DRV_USART_DRIVER_MODE="DYNAMIC"
CONFIG_DRV_USART_INTERRUPT_MODE=n
CONFIG_DRV_USART_BYTE_MODEL_SUPPORT=n
CONFIG_DRV_USART_READ_WRITE_MODEL_SUPPORT=y
CONFIG_DRV_USART_BUFFER_QUEUE_SUPPORT=y
CONFIG_DRV_USART_SUPPORT_TRANSMIT_DMA=n
CONFIG_DRV_USART_SUPPORT_RECEIVE_DMA=n
CONFIG_DRV_USART_INSTANCES_NUMBER=1
CONFIG_DRV_USART_CLIENTS_NUMBER=1
#
# from $HARMONY_VERSION_PATH/framework/driver/usart/config/drv_usart_idx.ftl
#
CONFIG_DRV_USART_INST_IDX0=y
CONFIG_DRV_USART_PERIPHERAL_ID_IDX0="USART_ID_2"
CONFIG_DRV_USART_BAUD_RATE_IDX0=115200
CONFIG_DRV_USART_OPER_MODE_IDX0="DRV_USART_OPERATION_MODE_NORMAL"
CONFIG_DRV_USART_INIT_FLAG_WAKE_ON_START_IDX0=n
CONFIG_DRV_USART_INIT_FLAG_AUTO_BAUD_IDX0=n
CONFIG_DRV_USART_INIT_FLAG_STOP_IN_IDLE_IDX0=n
CONFIG_DRV_USART_BRG_CLOCK_IDX0="80000000"
CONFIG_DRV_USART_LINE_CNTRL_IDX0="DRV_USART_LINE_CONTROL_8NONE1"
CONFIG_DRV_USART_HANDSHAKE_MODE_IDX0="DRV_USART_HANDSHAKE_NONE"
CONFIG_DRV_USART_XMIT_QUEUE_SIZE_IDX0=10
CONFIG_DRV_USART_RCV_QUEUE_SIZE_IDX0=10
CONFIG_DRV_USART_POWER_STATE_IDX0="SYS_MODULE_POWER_RUN_FULL"
#
# from $HARMONY_VERSION_PATH/framework/driver/wifi/config/drv_wifi.hconfig
#
CONFIG_USE_DRV_WIFI=n
#
# from $HARMONY_VERSION_PATH/framework/gfx/config/gfx.hconfig
#
CONFIG_USE_GFX_STACK=n
#
# from $HARMONY_VERSION_PATH/framework/gfx/config/gfx_segger.hconfig
#
CONFIG_USE_SEGGER_EMWIN=n
#
# from $HARMONY_VERSION_PATH/framework/math/dsp/config/dsp.hconfig
#
CONFIG_USE_DSP=n
#
# from $HARMONY_VERSION_PATH/framework/math/libq/config/libq.hconfig
#
CONFIG_USE_LIBQ_C=n
#
# from $HARMONY_VERSION_PATH/framework/net/pres/config/net_pres.hconfig
#
CONFIG_NET_PRES_USE=n
#
# from $HARMONY_VERSION_PATH/framework/osal/config/osal.hconfig
#
CONFIG_USE_OSAL=y
#
# from $HARMONY_VERSION_PATH/framework/peripheral/config/peripheral.hconfig
#
CONFIG_PERIPHERAL_LIB=y
#
# from $HARMONY_VERSION_PATH/framework/sample/config/sample_module.hconfig
#
CONFIG_USE_SAMPLE_MODULE=n
#
# from $HARMONY_VERSION_PATH/framework/system/clk/config/sys_clk.hconfig
#
CONFIG_USE_SYS_CLK=y
CONFIG_SYS_CLK_MODE="STATIC"
CONFIG_SYS_CLK_PBDIV0_OVERRIDE=n
CONFIG_SYS_CLK_PBDIV0_MX="DIV_1"
CONFIG_SYS_CLK_CONFIG_PRIMARY_XTAL="8000000"
CONFIG_SYS_CLK_CONFIG_SECONDARY_XTAL="32768"
CONFIG_SYS_CLK_FREQ="80000000"
CONFIG_SYS_CLK_PBCLK_FREQ="80000000"
CONFIG_SYS_CLK_UPLL_BEFORE_DIV2_FREQ="48000000"
#
# from $HARMONY_VERSION_PATH/framework/system/command/config/sys_command.hconfig
#
CONFIG_USE_SYS_COMMAND=y
CONFIG_COMMAND_PRINT_BUFFER_SIZE=512
CONFIG_REMAP_SYS_DEBUG_MESSAGE=y
CONFIG_REMAP_SYS_CONSOLE_MESSAGE=y
#
# from $HARMONY_VERSION_PATH/framework/system/common/config/sys_common.hconfig
#
CONFIG_USE_SYS_COMMON=y
CONFIG_SYS_BUFFER=n
CONFIG_SYS_QUEUE=n
#
# from $HARMONY_VERSION_PATH/framework/system/console/config/sys_console.hconfig
#
CONFIG_USE_SYS_CONSOLE=y
CONFIG_SYS_CONSOLE_MODE="DYNAMIC"
CONFIG_SYS_CONSOLE_OVERRIDE_STDIO=y
CONFIG_SYS_CONSOLE_INSTANCES_NUMBER_DYNAMIC=1
CONFIG_SYS_CONSOLE_SOURCE_IDX0="UART_CONSOLE"
CONFIG_SYS_CONSOLE_USE_UART_INSTANCE=0
CONFIG_SYS_CONSOLE_UART_RD_QUEUE_DEPTH=1
CONFIG_SYS_CONSOLE_UART_WR_QUEUE_DEPTH=64
#
# from $HARMONY_VERSION_PATH/framework/system/debug/config/sys_debug.hconfig
#
CONFIG_USE_SYS_DEBUG=y
CONFIG_SYS_ERR_LEVEL="SYS_ERROR_FATAL"
CONFIG_DEBUG_PRINT_BUFFER_SIZE=512
#
# from $HARMONY_VERSION_PATH/framework/system/devcon/config/sys_devcon.hconfig
#
CONFIG_USE_SYS_DEVCON=y
CONFIG_SYS_DEVCON_USE_JTAG=n
CONFIG_SYS_DEVCON_USE_TRACE=n
#
# from $HARMONY_VERSION_PATH/framework/system/dma/config/sys_dma.hconfig
#
CONFIG_USE_SYS_DMA=n
#
# from $HARMONY_VERSION_PATH/framework/system/fs/config/sys_fs.hconfig
#
CONFIG_USE_SYS_FS=n
#
# from $HARMONY_VERSION_PATH/framework/system/int/config/sys_int.hconfig
#
CONFIG_USE_SYS_INT=y
CONFIG_USE_EXT_INT=n
#
# from $HARMONY_VERSION_PATH/framework/system/msg/config/sys_msg.hconfig
#
CONFIG_USE_SYS_MSG=n
#
# from $HARMONY_VERSION_PATH/framework/system/ports/config/sys_ports.hconfig
#
CONFIG_USE_SYS_PORTS=y
CONFIG_SYS_PORTS_IMPLEMENTATION="STATIC"
CONFIG_COMPONENT_PACKAGE="TQFP"
CONFIG_SYS_PORTS_CN=n
CONFIG_USE_SYS_PORTS_CN_INTERRUPT=n
CONFIG_SYS_PORT_ADPCFG=0xffff
CONFIG_SYS_PORT_CNEN=0x0
CONFIG_SYS_PORT_CNPU=0x0
#
# from $HARMONY_VERSION_PATH/framework/system/ports/config/sys_ports_idx.ftl
#
CONFIG_USE_PORT_A=y
CONFIG_SYS_PORT_A_TRIS=0xc680
CONFIG_SYS_PORT_A_LAT=0x0
CONFIG_SYS_PORT_A_ODC=0x0
CONFIG_USE_PORT_B=y
CONFIG_SYS_PORT_B_TRIS=0x20
CONFIG_SYS_PORT_B_LAT=0x0
CONFIG_SYS_PORT_B_ODC=0x0
CONFIG_SYS_PORT_C_TRIS=0xf01e
CONFIG_SYS_PORT_C_LAT=0x0
CONFIG_SYS_PORT_C_ODC=0x0
CONFIG_SYS_PORT_D_TRIS=0xffff
CONFIG_SYS_PORT_D_LAT=0x0
CONFIG_SYS_PORT_D_ODC=0x0
CONFIG_SYS_PORT_E_TRIS=0x3ff
CONFIG_SYS_PORT_E_LAT=0x0
CONFIG_SYS_PORT_E_ODC=0x0
CONFIG_SYS_PORT_F_TRIS=0x313f
CONFIG_SYS_PORT_F_LAT=0x0
CONFIG_SYS_PORT_F_ODC=0x0
CONFIG_SYS_PORT_G_TRIS=0xf3cf
CONFIG_SYS_PORT_G_LAT=0x0
CONFIG_SYS_PORT_G_ODC=0x0
#
# from $HARMONY_VERSION_PATH/framework/system/random/config/sys_random.hconfig
#
CONFIG_USE_SYS_RANDOM=y
CONFIG_SYS_RANDOM_CRYPTO_SEED_SIZE=32
CONFIG_SYS_RANDOM_USE_CRYPTO_STRENGTH=n
#
# from $HARMONY_VERSION_PATH/framework/system/reset/config/sys_reset.hconfig
#
CONFIG_USE_SYS_RESET=y
#
# from $HARMONY_VERSION_PATH/framework/system/rtcc/config/sys_rtcc.hconfig
#
CONFIG_USE_SYS_RTCC=n
#
# from $HARMONY_VERSION_PATH/framework/system/touch/config/sys_touch.hconfig
#
CONFIG_USE_SYS_TOUCH=n
#
# from $HARMONY_VERSION_PATH/framework/system/tmr/config/sys_tmr.hconfig
#
CONFIG_USE_SYS_TMR=y
CONFIG_SYS_TMR_POWER_STATE="SYS_MODULE_POWER_RUN_FULL"
CONFIG_SYS_TMR_DRIVER_INDEX="DRV_TMR_INDEX_0"
CONFIG_SYS_TMR_MAX_CLIENT_OBJECTS=5
CONFIG_SYS_TMR_FREQUENCY=1000
CONFIG_SYS_TMR_FREQUENCY_TOLERANCE=10
CONFIG_SYS_TMR_UNIT_RESOLUTION=10000
CONFIG_SYS_TMR_CLIENT_TOLERANCE=10
CONFIG_SYS_TMR_INTERRUPT_NOTIFICATION=n
#
# from $HARMONY_VERSION_PATH/framework/system/wdt/config/sys_wdt.hconfig
#
CONFIG_USE_SYS_WDT=n
#
# from $HARMONY_VERSION_PATH/framework/test/config/test.hconfig
#
CONFIG_USE_TEST_HARNESS=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tcpip_stack.hconfig
#
CONFIG_USE_TCPIP_STACK=y
CONFIG_TCPIP_STACK_USE_IPV4=y
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/ip.hconfig
#
CONFIG_TCPIP_IPV4_FRAGMENTATION=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tcpip_stack.hconfig
#
CONFIG_TCPIP_STACK_USE_IPV6=n
CONFIG_TCPIP_USE_TCP=y
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tcp.hconfig
#
CONFIG_TCPIP_TCP_MAX_SEG_SIZE_TX=1460
CONFIG_TCPIP_TCP_MAX_SEG_SIZE_RX_LOCAL=1460
CONFIG_TCPIP_TCP_MAX_SEG_SIZE_RX_NON_LOCAL=536
CONFIG_TCPIP_TCP_SOCKET_DEFAULT_TX_SIZE=512
CONFIG_TCPIP_TCP_SOCKET_DEFAULT_RX_SIZE=512
CONFIG_TCPIP_TCP_DYNAMIC_OPTIONS=y
CONFIG_TCPIP_TCP_START_TIMEOUT_VAL=1000
CONFIG_TCPIP_TCP_DELAYED_ACK_TIMEOUT=100
CONFIG_TCPIP_TCP_FIN_WAIT_2_TIMEOUT=5000
CONFIG_TCPIP_TCP_KEEP_ALIVE_TIMEOUT=10000
CONFIG_TCPIP_TCP_CLOSE_WAIT_TIMEOUT=200
CONFIG_TCPIP_TCP_MAX_RETRIES=5
CONFIG_TCPIP_TCP_MAX_UNACKED_KEEP_ALIVES=6
CONFIG_TCPIP_TCP_MAX_SYN_RETRIES=3
CONFIG_TCPIP_TCP_AUTO_TRANSMIT_TIMEOUT_VAL=40
CONFIG_TCPIP_TCP_WINDOW_UPDATE_TIMEOUT_VAL=200
CONFIG_TCPIP_TCP_MAX_SOCKETS=10
CONFIG_TCPIP_TCP_TASK_TICK_RATE=5
CONFIG_TCPIP_TCP_MSL_TIMEOUT=0
CONFIG_TCPIP_TCP_QUIET_TIME=0
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tcpip_stack.hconfig
#
CONFIG_TCPIP_USE_UDP=y
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/udp.hconfig
#
CONFIG_TCPIP_UDP_MAX_SOCKETS=10
CONFIG_TCPIP_UDP_SOCKET_DEFAULT_TX_SIZE=512
CONFIG_TCPIP_UDP_USE_TX_CHECKSUM=y
CONFIG_TCPIP_UDP_USE_RX_CHECKSUM=y
CONFIG_TCPIP_UDP_SOCKET_DEFAULT_TX_QUEUE_LIMIT=3
CONFIG_TCPIP_UDP_SOCKET_DEFAULT_RX_QUEUE_LIMIT=3
CONFIG_TCPIP_UDP_USE_POOL_BUFFERS=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tcpip_stack.hconfig
#
CONFIG_TCPIP_STACK_NETWORK_CONFIG_NUMBER=1
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/network_config_idx.ftl
#
CONFIG_TCPIP_STACK_NETWORK_CONFIG_IDX0=y
CONFIG_TCPIP_NETWORK_DEFAULT_INTERFACE_NAME_IDX0="ENCX24J600"
CONFIG_TCPIP_NETWORK_DEFAULT_HOST_NAME_IDX0="MCHPBOARD_E"
CONFIG_TCPIP_NETWORK_DEFAULT_MAC_ADDR_IDX0=""
CONFIG_TCPIP_NETWORK_DEFAULT_IP_ADDRESS_IDX0=""
CONFIG_TCPIP_NETWORK_DEFAULT_IP_MASK_IDX0="255.255.255.0"
CONFIG_TCPIP_NETWORK_DEFAULT_GATEWAY_IDX0=""
CONFIG_TCPIP_NETWORK_DEFAULT_DNS_IDX0=""
CONFIG_TCPIP_NETWORK_DEFAULT_SECOND_DNS_IDX0="0.0.0.0"
CONFIG_TCPIP_NETWORK_DEFAULT_POWER_MODE_IDX0="full"
CONFIG_TCPIP_NETWORK_INTERFACE_FLAG_DHCP_CLIENT_IDX0=y
CONFIG_TCPIP_NETWORK_INTERFACE_FLAG_ZCLL_IDX0=n
CONFIG_TCPIP_NETWORK_INTERFACE_FLAG_DHCP_SERVER_IDX0=n
CONFIG_TCPIP_NETWORK_INTERFACE_FLAG_DNS_CLIENT_IDX0=y
CONFIG_TCPIP_NETWORK_INTERFACE_FLAG_DNS_SERVER_IDX0=n
CONFIG_TCPIP_NETWORK_DEFAULT_MAC_DRIVER_IDX0="DRV_ENCX24J600_MACObject"
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tcpip_stack.hconfig
#
CONFIG_TCPIP_STACK_TICK_RATE=5
CONFIG_TCPIP_STACK_USER_NOTIFICATION=n
CONFIG_TCPIP_STACK_DOWN_OPERATION=y
CONFIG_TCPIP_STACK_IF_UP_DOWN_OPERATION=y
CONFIG_TCPIP_STACK_CONFIGURATION_SAVE_RESTORE=y
CONFIG_TCPIP_STACK_SECURE_PORT_ENTRIES=10
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tcpip_heap.hconfig
#
CONFIG_TCPIP_USE_HEAP=y
CONFIG_TCPIP_STACK_USE_HEAP_CONFIG="TCPIP_STACK_HEAP_TYPE_INTERNAL_HEAP"
CONFIG_TCPIP_STACK_MALLOC_FUNC="malloc"
CONFIG_TCPIP_STACK_CALLOC_FUNC="calloc"
CONFIG_TCPIP_STACK_FREE_FUNC="free"
CONFIG_TCPIP_STACK_HEAP_USE_FLAGS="TCPIP_STACK_HEAP_FLAG_ALLOC_UNCACHED"
CONFIG_TCPIP_STACK_HEAP_USAGE_CONFIG="TCPIP_STACK_HEAP_USE_DEFAULT"
CONFIG_TCPIP_STACK_SUPPORTED_HEAPS=1
CONFIG_TCPIP_STACK_DRAM_SIZE=39250
CONFIG_TCPIP_STACK_DRAM_RUN_LIMIT=2048
CONFIG_TCPIP_STACK_DRAM_DEBUG_ENABLE=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/arp.hconfig
#
CONFIG_TCPIP_ARP_CACHE_ENTRIES=5
CONFIG_TCPIP_ARP_CACHE_DELETE_OLD=y
CONFIG_TCPIP_ARP_CACHE_SOLVED_ENTRY_TMO=1200
CONFIG_TCPIP_ARP_CACHE_PENDING_ENTRY_TMO=60
CONFIG_TCPIP_ARP_CACHE_PENDING_RETRY_TMO=2
CONFIG_TCPIP_ARP_CACHE_PERMANENT_QUOTA=50
CONFIG_TCPIP_ARP_CACHE_PURGE_THRESHOLD=75
CONFIG_TCPIP_ARP_CACHE_PURGE_QUANTA=1
CONFIG_TCPIP_ARP_CACHE_ENTRY_RETRIES=3
CONFIG_TCPIP_ARP_GRATUITOUS_PROBE_COUNT=1
CONFIG_TCPIP_ARP_TASK_PROCESS_RATE=2
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/berkeley_api.hconfig
#
CONFIG_TCPIP_STACK_USE_BERKELEY_API=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/dhcp.hconfig
#
CONFIG_TCPIP_STACK_USE_DHCP_CLIENT=y
CONFIG_TCPIP_DHCP_TIMEOUT=2
CONFIG_TCPIP_DHCP_TASK_TICK_RATE=5
CONFIG_TCPIP_DHCP_CLIENT_ENABLED=y
CONFIG_TCPIP_DHCP_HOST_NAME_SIZE=20
CONFIG_TCPIP_DHCP_CLIENT_CONNECT_PORT=68
CONFIG_TCPIP_DHCP_SERVER_LISTEN_PORT=67
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/dhcps.hconfig
#
CONFIG_TCPIP_STACK_USE_DHCP_SERVER=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/dns.hconfig
#
CONFIG_TCPIP_USE_DNS_CLIENT=y
CONFIG_TCPIP_DNS_CLIENT_SERVER_TMO=60
CONFIG_TCPIP_DNS_CLIENT_TASK_PROCESS_RATE=200
CONFIG_TCPIP_DNS_CLIENT_CACHE_ENTRIES=5
CONFIG_TCPIP_DNS_CLIENT_CACHE_ENTRY_TMO=0
CONFIG_TCPIP_DNS_CLIENT_CACHE_PER_IPV4_ADDRESS=5
CONFIG_TCPIP_DNS_CLIENT_CACHE_PER_IPV6_ADDRESS=1
CONFIG_TCPIP_DNS_CLIENT_ADDRESS_TYPE="IP_ADDRESS_TYPE_IPV4"
CONFIG_TCPIP_DNS_CLIENT_CACHE_DEFAULT_TTL_VAL=1200
CONFIG_TCPIP_DNS_CLIENT_CACHE_UNSOLVED_ENTRY_TMO=10
CONFIG_TCPIP_DNS_CLIENT_LOOKUP_RETRY_TMO=5
CONFIG_TCPIP_DNS_CLIENT_MAX_HOSTNAME_LEN=32
CONFIG_TCPIP_DNS_CLIENT_MAX_SELECT_INTERFACES=4
CONFIG_TCPIP_DNS_CLIENT_DELETE_OLD_ENTRIES=y
CONFIG_TCPIP_DNS_CLIENT_USER_NOTIFICATION=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/dnss.hconfig
#
CONFIG_TCPIP_USE_DNSS=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/ddns.hconfig
#
CONFIG_TCPIP_USE_DDNS=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/ftp.hconfig
#
CONFIG_TCPIP_USE_FTP_MODULE=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/http.hconfig
#
CONFIG_TCPIP_STACK_USE_HTTP_SERVER=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/http_net.hconfig
#
CONFIG_TCPIP_STACK_USE_HTTP_NET_SERVER=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/icmp.hconfig
#
CONFIG_TCPIP_STACK_USE_ICMPV4=y
CONFIG_TCPIP_STACK_USE_ICMP_SERVER=y
CONFIG_TCPIP_STACK_USE_ICMP_CLIENT=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/nbns.hconfig
#
CONFIG_TCPIP_USE_NBNS=y
CONFIG_TCPIP_NBNS_TASK_TICK_RATE=110
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tcpip_reboot.hconfig
#
CONFIG_TCPIP_USE_REBOOT_SERVER=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/smtp.hconfig
#
CONFIG_TCPIP_USE_SMTP_CLIENT=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/smtpc.hconfig
#
CONFIG_TCPIP_USE_SMTPC_CLIENT=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/snmp.hconfig
#
CONFIG_TCPIP_USE_SNMP=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/sntp.hconfig
#
CONFIG_TCPIP_USE_SNTP_CLIENT=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/telnet.hconfig
#
CONFIG_TCPIP_USE_TELNET=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/zeroconf.hconfig
#
CONFIG_TCPIP_USE_LINK_ZERO_CONFIG=y
CONFIG_TCPIP_ZC_WARN_ZCLL=n
CONFIG_TCPIP_ZC_INFO_ZCLL=n
CONFIG_TCPIP_ZC_DEBUG_ZCLL=n
CONFIG_TCPIP_ZC_LL_PROBE_WAIT=1
CONFIG_TCPIP_ZC_LL_PROBE_MIN=1
CONFIG_TCPIP_ZC_LL_PROBE_MAX=2
CONFIG_TCPIP_ZC_LL_PROBE_NUM=3
CONFIG_TCPIP_ZC_LL_ANNOUNCE_WAIT=2
CONFIG_TCPIP_ZC_LL_ANNOUNCE_NUM=2
CONFIG_TCPIP_ZC_LL_ANNOUNCE_INTERVAL=2
CONFIG_TCPIP_ZC_LL_MAX_CONFLICTS=10
CONFIG_TCPIP_ZC_LL_RATE_LIMIT_INTERVAL=60
CONFIG_TCPIP_ZC_LL_DEFEND_INTERVAL=10
CONFIG_TCPIP_ZC_LL_IPV4_LLBASE=0xa9fe0100
CONFIG_TCPIP_ZC_LL_IPV4_LLBASE_MASK=0x0000FFFF
CONFIG_TCPIP_ZC_LL_TASK_TICK_RATE=333
CONFIG_TCPIP_USE_MULTI_CAST_DNS_ZERO_CONFIG=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tcpip_announce.hconfig
#
CONFIG_TCPIP_USE_ANNOUNCE=y
CONFIG_TCPIP_ANNOUNCE_MAX_PAYLOAD=512
CONFIG_TCPIP_ANNOUNCE_TASK_RATE=333
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/iperf.hconfig
#
CONFIG_TCPIP_USE_IPERF=n
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tcpip_cmd.hconfig
#
CONFIG_TCPIP_STACK_USE_COMMANDS=y
CONFIG_TCPIP_STACK_COMMANDS_STORAGE_ENABLE=n
CONFIG_TCPIP_STACK_COMMANDS_ICMP_ECHO_REQUESTS=4
CONFIG_TCPIP_STACK_COMMANDS_ICMP_ECHO_REQUEST_DELAY=1000
CONFIG_TCPIP_STACK_COMMANDS_ICMP_ECHO_TIMEOUT=5000
CONFIG_TCPIP_STACK_COMMANDS_WIFI_ENABLE=n
CONFIG_TCPIP_STACK_COMMANDS_ICMP_ECHO_REQUEST_BUFF_SIZE=2000
CONFIG_TCPIP_STACK_COMMANDS_ICMP_ECHO_REQUEST_DATA_SIZE=100
#
# from $HARMONY_VERSION_PATH/framework/tcpip/config/tftpc.hconfig
#
CONFIG_TCPIP_USE_TFTPC_MODULE=n
#
# from $HARMONY_VERSION_PATH/framework/usb/config/usb.hconfig
#
CONFIG_USE_USB_STACK=n
#
# from $HARMONY_VERSION_PATH/bsp/config/bsp.hconfig
#
CONFIG_USE_BSP=y
#
# from $HARMONY_VERSION_PATH/bsp/config/DS60001156.hconfig
#
CONFIG_BSP_PIC32MX_ETH_SK=n
CONFIG_BSP_PIC32MX_ETH_SK2=n
CONFIG_BSP_PIC32MX_PCAP_DB=n
CONFIG_BSP_PIC32MX_USB_SK2=n
CONFIG_BSP_PIC32MX_USB_SK2_LCC_PICTAIL_QVGA=n
CONFIG_BSP_PIC32MX_USB_SK2_LCC_PICTAIL_WQVGA=n
CONFIG_BSP_PIC32MX_USB_SK2_MEB=n
CONFIG_BSP_PIC32MX_USB_SK2_S1D_PICTAIL_VGA=n
CONFIG_BSP_PIC32MX_USB_SK2_S1D_PICTAIL_WQVGA=n
CONFIG_BSP_PIC32MX_USB_SK2_S1D_PICTAIL_WVGA=n
CONFIG_BSP_PIC32MX_USB_SK2_SSD_PICTAIL_QVGA=n
CONFIG_BSP_PIC32MX795_PIM_E16=y
CONFIG_BSP_CHIPKIT_WF32=n
CONFIG_BSP_WIFI_G_DB=n
#
# from $HARMONY_VERSION_PATH/third_party/rtos/config/rtos.hconfig
#
CONFIG_USE_3RDPARTY_RTOS=n
#
# from $HARMONY_VERSION_PATH/third_party/tcpip/config/wolfssl.hconfig
#
CONFIG_USE_3RDPARTY_WOLFSSL=n
#
# from $HARMONY_VERSION_PATH/third_party/tcpip/iniche/config/embtcp.hconfig
#
CONFIG_IN_EMB_TCPIP_USE_TCP=n
#
# from $HARMONY_VERSION_PATH/third_party/tcpip/iniche/config/embdual.hconfig
#
CONFIG_IN_EMB_DUAL_USE_TCP=n
#
# from $HARMONY_VERSION_PATH/third_party/tcpip/iniche/config/stack.hconfig
#
CONFIG_IN_TCPIP=n
#
# from $HARMONY_VERSION_PATH/third_party/gfx/config/gfxtp.hconfig
#
CONFIG_3RDPARTY_SEGGER_EMWIN_LIBRARY=n
#
# from $HARMONY_VERSION_PATH/config/harmony.hconfig
#
CONFIG_DEVICE_CONFIGURATION=y
#
# from $HARMONY_VERSION_PATH/utilities/mhc/config/PIC32MX795F512L.hconfig
#
CONFIG_USERID=0xffff
CONFIG_FSRSSEL="PRIORITY_7"
CONFIG_FMIIEN="OFF"
CONFIG_FETHIO="OFF"
CONFIG_FCANIO="OFF"
CONFIG_FUSBIDIO="OFF"
CONFIG_FVBUSONIO="OFF"
CONFIG_FPLLIDIV="DIV_2"
CONFIG_FPLLMUL="MUL_20"
CONFIG_UPLLIDIV="DIV_2"
CONFIG_UPLLEN="ON"
CONFIG_FPLLODIV="DIV_1"
CONFIG_FNOSC="PRIPLL"
CONFIG_FSOSCEN="ON"
CONFIG_IESO="ON"
CONFIG_POSCMOD="XT"
CONFIG_OSCIOFNC="OFF"
CONFIG_FPBDIV="DIV_1"
CONFIG_FCKSM="CSECME"
CONFIG_WDTPS="PS1048576"
CONFIG_FWDTEN="OFF"
CONFIG_DEBUG="ON"
CONFIG_ICESEL="ICS_PGx2"
CONFIG_PWP="OFF"
CONFIG_BWP="OFF"
CONFIG_CP="OFF"
#
# from $HARMONY_VERSION_PATH/config/harmony.hconfig
#
CONFIG_PROJECT_STANDALONE=n
#
# from $HARMONY_VERSION_PATH/utilities/mhc/config/project.hconfig
#
CONFIG_XC32_HEAP="44960"
#
# from $HARMONY_VERSION_PATH/utilities/mhc/config/isa.hconfig
#
CONFIG_ISA_MIPS32_MODE=y
CONFIG_ISA_MIPS16_MODE=n
