# MarlinKimbra 3D Printer Firmware
<img align="right" src="Documentation/Logo/MarlinKimbra%20Logo%20GitHub.png" />

  * [Configuration & Compilation](/Documentation/Compilation.md)
  * Supported
    * [Features](/Documentation/Features.md)
    * [Hardware](/Documentation/Hardware.md)
    * [GCodes](/Documentation/GCodes.md)
  * Notes
    * [Auto Bed Leveling](/Documentation/BedLeveling.md)
    * [Filament Sensor](/Documentation/FilamentSensor.md)
    * [Ramps Servo Power](/Documentation/RampsServoPower.md)
    * [LCD Language - Font - System](Documentation/LCDLanguageFont.md)
  * Version
    * [Change Log](/Documentation/changelog.md)


## Configurator Tool Online

http://marlinkimbra.it


## Quick Information

This version of Marlin was made to accommodate some requests made by the community RepRap Italy http://forums.reprap.org/index.php?349
The new features are:
A single Firmware for all types of printers; Cartesian, Delta, SCARA, CoreXY & CoreXZ.
The possibility of having only one hotend independently from the extruders that you have.
The addition of the 4th extruder.
System Management MKr4 for 4 extruders with just two drivers or two extruders with a driver only.
Management Multyextruder NPr2, 4/6 extruders with only two engines.
Adding commands to facilitate purging of hotend. 
Step per unit varied for each extruder as well as the feedrate.
The addition of a different feedrate for retraction. 
Adding Debug Dryrun used by repetier.
Add total Power on time write in EEPROM

## Credits

The current MarlinKimbra dev team consists of:
 - MagoKimbra - Alberto Cotronei (https://github.com/MagoKimbra)

More features have been added by:
  - simone97 (https://github.com/simone97)
  -

## License

Marlin is published under the [GPL license](/Documentation/COPYING.md) because I believe in open development.
Please do not use this code in products (3D printers, CNC etc) that are closed source or are crippled by a patent.
